**ANNEXURES**

**ZEAL EX**

|  |
| --- |
| **Zeal Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 50 ±5 Km/hr |
| **Max Loading Capacity** | 150 Kg |
| **Range**  | 85 +/- 5 Kms |
| **Vehicle** | **Kerb Weight** | 78 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance** | 145 mm |
| **Wheelbase** | 1235 mm |
| **Type** | BLDC Motor |
| **Voltage** | 60V |
| **Continuous Power** | 1200W |
| **Battery** | **Battery** |
| **Model** | 60V-30Ah, Li-ion |
| **Unique Salient Features** | **Remote key set, Anti-theft Alarm, Find my scooter** |  |
| **USB Charging** |  |

**Reo Plus LA**

|  |
| --- |
| **Reo Plus LA Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 25 Km/hr |
| **Max Loading Capacity** | 130 Kg |
| **Range**  | 55 -60 Kms |
| **Vehicle** | **Kerb Weight** | 87 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance**  | 145 mm |
| **Wheelbase** | 1235 mm |
| **Brake** | Mechanical Drum -110mm |
| **Model** | 48V-27Ah, LA |

**Reo Plus Lithium Ion**

|  |
| --- |
| **Reo Plus Li Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 25 Km/hr |
| **Max Loading Capacity** | 130 Kg |
| **Range**  | 60 - 65 Kms |
| **Vehicle** | **Kerb Weight** | 68 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance**  | 145 mm |
| **Wheelbase** | 1235 mm |
| **Dimensions (LXWXH) mm** | 1730\*660\*1200 |
| **Brake** | Mechanical Drum -110mm |
| **Variants** | **Reo Li** |
| **Unique Salient Features** | **Handbag Hook** |  |
| **Stylish Mirrors** |  |
| **USB Charging** |  |
| **Ignition Switch** |  |
| **LED Head Light** |  |
| **Aesthetic Floor Mat**  |  |

**Reo Elite LA**

|  |
| --- |
| **ELITE LA Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 25 Km/hr |
| **Max Loading Capacity** | 130 Kg |
| **Range**  | 55- 60 Kms |
| **Vehicle** | **Kerb Weight** | 86 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance**  | 130 mm |
| **Wheelbase** | 1270 mm |
| **Dimensions (LXWXH) mm** | 1670X640X1100 |
| **Brake** | Mechanical Drum -110mm |
| **Variants** | **Elite LA** |
| **Unique Salient Features** | **Handbag Hook**  |  |
| **USB Charging** |   |
| **LED Head Light** |   |
| **Stylish Floor Mat**  |   |
| **Digital display** |   |

**Reo Elite Lithium Ion**

|  |
| --- |
| **ELITE Li Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 25 Km/hr |
| **Max Loading Capacity** | 130 Kg |
| **Range**  | 60 - 65 Kms |
| **Vehicle** | **Kerb Weight** | 68 kgs |
| **Pay load capacity -Normal** | 130 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance**  | 130 mm |
| **Wheelbase** | 1270 mm |
| **Dimensions (LXWXH) mm** | 1670X640X1100 |
| **Brake** | Mechanical Drum -110mm |
| **Variants** | **Elite LA** |
| **Unique Salient Features** | **Handbag Hook**  |  |
| **USB Charging** |   |
| **LED Head Light** |   |
| **Stylish Floor Mat**  |   |
| **Digital display** |   |

**Magnus 60 Slow Speed**

|  |
| --- |
| **Magnus 60 Customer Specification** |
| **Parameter** | **Specification** |
| **Performance** | **Rated Speed** | 25 Km/hr |
| **Max Loading Capacity** | 130 Kg |
| **Range**  | 60- 65 Kms |
| **Vehicle** | **Kerb Weight** | 94 kgs |
| **Suspension** | Front-TelescopicRear-Coil Spring |
| **Ground Clearance**  | 160 mm |
| **Wheelbase** | 1415 mm |
| **Dimensions (LXWXH) mm** | 1880X710X1190 |
| **Brake** | Mechanical Drum -110mm CBS  |
| **Unique Salient Features**  |
| **Digital display** |    |
| **Microcontroller based Charger for battery protection** |  |
| **Front glove box** |    |
| **Durable shock absorbers** |    |
| **Junction box for easy rear wheel service** |    |
| **Carry bag hook** |    |